| # Older changes

#### 1.0.3 04-February-2015

- First public version

#### 1.0.4 06-February-2015

- Fixed: Continent is updated now correctly in: Menu–>Logbook–>Recalculate DXCCs - Tnx W0DJC
- Fixed: Problem during HamQTH.com query after changes at the server site, Tnx OK2CQR

#### 1.0.5 20-February-2015

- Fixed: Crash when viewing an empty dx-spot database - Tnx DH2PAF
- Fixed: Time intervall for dx spot database queries was always fixed to e weeks, regardless of selection
- New: Label size Avery 3474 added for QSL label printing
- New: Better LoTW preferences, RUMlog reads now used callsigns and station locations from the tqsl settings
- New: ADIF tag OPERATOR added as export/import option for user defined fields
- New: P3 Control window: Menu–>Transceiver–>P3/PX3 control Use P3 Firmware >= 1.35

#### 1.0.6 21-February-2015

- Fixed: CAT for Kenwood is working again - Tnx DH6YMC and N1JM
- Fixed: rst will be set now according TRX mode - Tnx DH6YMC
- New: 33cm band added
- New: Table for supported bands/frequencies added under: Preferences–>QRGs

#### 1.0.7 26-February-2015

- Fixed: HamQTH.com shows now correct US State and County
- New: Label size Avery 4781 added for QSL label printing
- New: Text alignment options added for QSL label print out

#### 1.0.8 7-March-2015

If you are a LoTW user, you have to enter the path to the .tqsl folder! See the Lotw preferences.

- Fixed: qrz.com shows now the “addr1” information as well - Tnx DF4WA
- Fixed: CAT control will be disabled now before falling into sleep, this prevents problems after wake up in some configurations
- Fixed: Edited QSOs are shown now correct - Tnx KK6FNK
- Fixed: Text alignment on QSL label is affected now correct by settings - Tnx KK6FNK
- New: Label size Avery 5163 added for QSL label printing
- New: A click in a QSO row in the LoTW or eQSL In Window shows now all QSOs with this station in the Logging Window

#### 1.0.9 11-March-2015

- Fixed Better compatibility for 10.9, was not fixed in 1.0.8 - Tnx K4ZRJ & AL7EK
- Fixed: Statistics are corrected now for “invalid operation” All invalids count now. Recalculate your statistics to update: Menu–>Logbook–>Recalculate DXCCs Use the search options and select the invalids first. - Tnx NF4L
- New: You can choose now you own text- and background colors for dx spots in Preferences–>DX Alarm–>Set colors

#### 1.1 26-March-2015

Please check your settings in Preferences–>DX Alarm! There are major changes.

- Fixed: KX3 don’t send a @ in CW after pressing the Escape key - Tnx DK5LP
- Fixed: Better DXCC recognition for portable Operationen for 3B, EA, HC, TI, UA, ZL and ZS - Tnx LA0FA
- Fixed: LoTW Upload with satellietes QSOs corrected - Tnx EA2CQ
- Fixed: qrz.com shows all station images correct now - Tnx W0DJC
- New: DX Spots for New Ones can be spoken now - See also Preferences–>DX Alarm
- New: The opening of an extra spot window for searched stations is optional now
- New: Support for FTdx3000 - Tnx N2TSQ
- New: Support for FTdx5000 - Tnx LA0FA
- New: More AppleScript support for JT-Bridge - Tnx SM0THU
- New: A click into the bandmap on the call sign printout sets the TRX and the logging fields now
- New: You can take over data from previous QSOs during logging, see Preferences–>Databases for settings and the link “QSO Entry fields”
- New: A “No zoom” option added in the large map window, this prevents the map to zoom in automatically.
- New: Use of OS-X Notification Centre, use the System Preferences for further settings
- New: Toggle option: Menu–>Logbook–>Clear after QSY: clears all fields, when the VFO is tuned 1 kHz away
- New: More edit options when editing multiple QSOs with the same station
- New: DX spot window will be filled with data after “show/dx” as well
- New: All times are in 24 hours format now, regardless of system settings

#### 1.2 17-May-2015

- Fixed: DXCC computation for KG4 optimized - Tnx N1HO
- Fixed: IOTA reference for Oceania can now be entered correct - Tnx IK2EAE
- New: All areas currently located in the gray line can be listed in a separate table - See the link Miscellaneous Windows
- New: Support for Dymo Labelwriter format 57mm x 32mm - Tnx DL7XT
- New: Extended QSO search - See the link Miscellaneous Windows
- New: Support for FT-991 - Tnx DL4ABB
- New: Support for FTdx1200
- New: Dx Entity column added in the dx-spot tables
- New: Open unlimited number of band maps: Menu–>Window–>New Band Map
- New: Better CW window

#### 1.2.1 18-May-2015

- Fixed: CAT optimization for TS-2000 - Tnx WK8A

#### 1.2.2 20-May-2015

- Fixed: Preferences for user defined fields - Tnx DL2RUM

#### 1.2.3 23-May-2015

- Fixed: Zones are shown now correct after double clicking a dx-spot - Tnx IK2EAE

#### 1.2.4 13-June-2015

- Fixed: CW window Info field are not any longer mirrored in the rst field - Tnx DH6YMC
- Fixed: OS X notifications take eQSL and LoTW users now into consideration - Tnx NY4I

#### 1.2.5 3-July-2015

- Fixed: Printed QSL label shows correct rst now - Tnx OE1HXS
- Fixed: QSO Search window will be updated after log changes - Tnx DK5LP
- New: Support for FT-1000MP Mark-V - Tnx OE3ASA
- New: qrz.com/HamQTH.com informationen can be shown now below the logging window

#### 1.2.6 13-July-2015

- Fixed: problems with Timeout errors during up- and download fixed
- Fixed: Graphical issues fixed at the top of the band map
- Fixed: Data take over by a click into a band map works more reliable now
- New: DX-spot colors will be updated now after logging or deleting a QSO
- New: Option added to define the table columns width behavior while resizing the table: Preferences–>General–>Logbook behavior

#### 2.0 1-October-2015

- Fixed: Extended QSO Search will take the QSO time now into consideration - this was undefined before and the results unexpected - Tnx N8XMS
- New: Contest and dx-ped module
- New: Support for a second transceiver
- New: Support for Ten Tec Orion - Tnx ON5YA
- New: Support for QSL label Avery 5161 (US-Letter, 1" x 4" , 2 x 10)
- New: ADIF tag STATION_CALLSIGN added for im- and export of user fields

#### 2.1 24-October-2015

- Fixed: Window Calculations - When the date is changed, the sun times for location B will be recalculated now - Tnx DL2RUM
- Fixed: Contestlog: Scoring corrected, due to an error in saving the correct dxcc entity
- Fixed: Scoring for WWDX corrected - Tnx K6LE
- New: Support for label Avery 3653 (42.4mm x 105mm at DIN A4 2 x 7)
- New: In the Terminal window you can connect now up to 4 dx-cluster
- New: QSOs can be color coded in the log tables - Tnx M0CLH
- New: Ukrainian DX Contest

#### 2.2 3-November-2015

- Fixed: Textlabels show correct text color now
- Fixed: Bug during CAT initialization removed - Tnx DG3YJB
- New: QSO table background color can be given now during logging
- New: Apple Script support for Paper QSL
- New: A new drawer window in the contest interface can show all possible control numbers (multipliers) - if applicable
- New: JA DX Contest
- New: OK/OM DX Contest
- New: ARRL 160m Contest
- New: ARRL 10m Contest
- New: LZ DX Contest
- New: DARC XMAS Contest
- New: Croatian CW Contest

#### 2.3 27-November-2015

- Fixed: No more crashes when receiving specific LoTW QSLs - Tnx DL7VDX
- New: CQ zone (WAZ) can be set as dx alarm
- New: ADIF tag TIME_ON added for user definable logging fields
- New: Direct sql QSO search for experts in the QSO Search Window
- New: Support for Avery 8162 (DIN A4, 99.1 x 33.9 mm, 2 x 8)
- New: RTTY Operation in the Contest Modul via Fldigi or K3/KX3 (Contest und DX-Pedition)
- New: DARC Corona Contest
- New: OK RTTY DX Contest
- New: Ten-Meter RTTY Contest
- New: USKA XMAS Contest
- New: USKA Helvetia Contest
- New: General Contest (no scoring)

#### 2.4 13-December-2015

- Fixed: Crash during Cabrillo output when using OS-X 10.9 - Tnx OE1HXS
- New: You can add data from HamQTH.com or qrz.com to logbook entries: Menu–>QSO–>Add QSO data
- New: All band tables in the dx-spot window include now a contextual menu in the header to show/hide columns
- New: Search Entities Window: Select one or multiple Entities in the result table to mark appropriate QSOs - Tnx EA5FY
- New: Print QSL label: As alternate, you can select the last free label for the first sheet to print - Tnx SQ2KLU
- New: Dymo Label 57mm x 32mm now optional with one QSO and two footer rows
- New: DARC 10m Contest
- New: North American QSO Party
- New: REF Contest
- New: Brandenburg-Berlin Contest
- New: CQWW 160m Contest
- New: UBA DX Contest

#### 2.5 20-January-2016

- Fixed: QSL Manager was missing in Global QSL ADIF file - Tnx DK5CM
- New: More CW options in the Log Preferences under the CW tab - you have to reset your settings
- New: “New one” dx-spots can be notified using Growl
- New: You can remove now a callsign from a band map using cmd mouse click
- New: Separate band map and dx spot windows for the contest module
- New: Memory pad for contest operation
- New: Audio recording and play back functions
- New: QSO Export funktion for SOTA database (version 2)
- New: Support for Avery 7163
- New: Introduction of a Contest Cheat database - Tnx DL6ER
- New: AppleScript support for read/write of State, QSO date & time, the four user fields and for the Use real time checkbox
- New: ARRL Int. DX Contest
- New: CQ WPX contests - CW/SSB/RTTY
- New: PACC Contest

#### 2.5.2 31-January-2016

- Fixed: No more crashes when using some brands of external sound cards - Tnx EA5CQ, NA4M
- Fixed: Failure fixed, where the Preferences Window was completely unresposible - Tnx EA5CQ, NA4M
- Fixed: Ivory Coast (TU) is back on the DXCC list - Tnx IT9CML

#### 2.5.3. 17-February-2016

- Fixed: 10.9 (Mavericks) users can edit QSOs now again - Tnx AA4GA
- Fixed: QSOs for SOTA export are sorted now by date and time - Tnx W6UB
- Fixed: Cabrillo file shows now the correct frequency, after editing the band - Tnx Bill, AE6JV
- Fixed: Camden County, NJ added to database - Tnx IT9CML
- New: Dymo Label 89mm x 36mm

#### 2.6 3-March-2016

- Fixed: Interface problem band map/dx spot and contest window fixed - Tnx BG5EEF & K6LE
- New: DX spot window can show now the State (W), Province (VE) or the DOK (DL). A dx alarm can be set. You have to load the database first: Menu–>Online–>Load contest cheat database
- New: Elecraft P3 window shows now controls to change the P3 display font size and to toggle the TX meters. P3 Firmware MCU 01.57 oder newer required.
- New: Russian DX Contest
- New: RSGB Commonwealth Contest
- New: DARC Oster Contest
- New: South America 10m Contest

#### 2.7 29-March-2016

- Fixed: US-State now shown correctly in the 6m dx-spot table - Tnx IK2EAE
- New: Support for Avery 7159
- New: Dymo label 1" x 2-1/8"
- New: Dymo label 2-1/8 x 4"
- New: For the incoming eQSL you can define now the time slot for QSO-QSL time matching in the Preferences under the LoTW/eQSL tab.
- New: UBA ON Contest
- New: UBA Spring Contest
- New: SPDX Contest
- New: CWops Contest -> reload the Contest Cheat Database from the Online menu
- New: YU DX Contest
- New: Yuri Gagarin Contest
- New: Worked All Provinces of China DX Contest

#### 2.8 30-April-2016

- Fixed: ADIF Import: Deprecated Enumeration ‘V’ for the tags LOTW_QSL_RCVD und QSL_RCVD are interpreted as ‘Y’ now - Tnx K3DCW
- Fixed: Correction in the WPX prefix calculation - Tnx IV3TMM
- New: Changes for newest microHAM Firmware (3.3 for DKII and 6.3 for MKII)
- New: 7th Call Area QSO Party
- New: CQ-M International DX Contest
- New: A.R.I. International DX Contest
- New: His Majesty The King of Spain Contest
- New: Hessen Contest
- New: Hamburg Contest

#### 2.9 27-May-2016

- Fixed: Contest logging was impossible, when there is an apostrophe in the Computer’s name - Tnx G4AWP
- Fixed: DX-Cluster Auto Connect works now in the first terminal tab as expected - Tnx IV4TMM
- Fixed: Main Logging Window: Recently added or deleted QSOs are shown now correct in the Search section - Tnx IV4TMM
- Fixed: Data take over from previous QSOs: The newest datas will be used now - settings are saved now correct - Tnx IV4TMM
- New: Elecraft KX2 support added, including full control window
- New: In a log table selected QSO or the results from a DXCC entity search can be presented on a map - See the QSO menu
- New: IARU Region 1 Fieldday
- New: RSGB CW National Field Day
- New: Worked All VK Shires
- New: Portugal Day Contest
- New: World Wide South America CW Contest
- New: All Asian DX Contest (CW & SSB)
- New: Ukrainian DX Digi Contest

#### 2.10 26-June-2016

- Change: The Fldigi preferences can be found now under the µHAM/Fldigi tab, no changes in function
- New: Support for QSL label Avery 8462 (1-1/3" x 4" at US-Letter 2 x 7)
- New: IC-7300 control window - select IC-7300 Ctrl as transceiver
- New: The eight CW memories for the IC-7300 can be edited –> Menu–>Transceiver–>Edit CW memory
- New: You can set the serial CAT port flow control lines to High, to power up the interface
- New: Option added to use a Bluetooth Low Energy Modul CAT interface
- New: Provisions made to use the internal CW keyers in IC-7100, 7300, 7410, 7700, 7850, 7851 and 9100
- New: DXCC search: option added to search for exclusively LoTW or paper confirmed entities
- New: Command added to set the Paper QSO Status for selected QSOs to -: Menu–>QSL–>Do not send QSL. This works in the Search Windows as well.
- New: RAC Canada Day Contest
- New: Venezuelan Independence Contest
- New: DL-DX RTTY Contest
- New: IARU HF Championship
- New: RSGB Low Power Contest
- New: RSGB IOTA Contest

#### 2.10.1 28-June-2016

- Fixed: Connection to Fldigi controls in the Preferences repaired
- New: User fields can be mapped now to ADIF tags “MY_SIG” and “MY_SIG_INFO” (Used for WWFF)

#### 2.11 22-July-2016

- Fixed: RUMlog toggles PTT for Fldigi, while Fldigi in in Tune mode - Tnx Jwahar, KC1CCR
- New: Callsign auto complete function in the Paper QSL In window
- New: In the separate Map window, you can add a grid square overlay
- New: In HamQTH.com or qrz.com found postal addresses can be used for address label printing - See Menu–>QSL
- New: Satellite list updated
- New: For the grid square you can save now up to 10 digits
- New: The local time zone can be used instead of utc, see Preferences–>General–>Logbook behavior
- New: QSO Note field can be prefilled with data from a previous QSO: Preferences–>Databases–>Fill entry fields with data from previous QSOs
- New: European HF Championship
- New: RDA Contest
- New: YO DX HF Contest
- New: KCJ Contest
- New: WAEDC CW/SSB/RTTY - including QTC traffic

#### 2.12 25-August-2016

- Fixed: The window Receive Paper QSLs shows the QSOs with the selected colour code now - Tnx Terry, M0CLH
- Fixed: Entry of a / for a received QTC is possible now - Tnx DL1RF
- New: Load, view and save eQSL images Menu–>QSL–>Load eQSL image
- New: Apple Script support for the contest interface
- New: Use the internal CW keyer in the TS-480 - Tnx DL7VDX
- New: IC-7300 Control Window: Scope reference level can be saved and restored by band (optional)
- New: IC-7300 Control Window: Scope fixed edges can be selected matching the actual frequency (optional)
- New: Open a Contest or Logbook file by double click it or drop a file over the application icon
- New: Support for label printer format 90mm x 29mm
- New: If the option Menu–>Logbook–>Show prev. QSOs selected, the logbook will not show any longer an empty table when the station isn’t in the log yet
- New: CAT support for FT-840
- New: RSGB SSB Field Day
- New: FOC QSO Party (Please reload the Contest Cheat Database: Menu–>Online–>Load contest cheat Database)
- New: Africa All Mode International DX Contest
- New: New England QSO Party

#### 2.13 25-September-2016

- Fixed: General Contest: Failure in creating the serial number fixed - Tnx DK1OM
- New: Option added for Fldigi PTT switching
- New: Commands added to save all downloaded eQSL images and to close all windows - See Menu–>QSL
- New: QSOs can be deleted now from the Search QSOs window
- New: IC-7300 Control: Auto Hold Funktion for the Scope Center Mode
- New: qrz.com queries ignore /P, /M, /AM, /MM and /QRP
- Neu: Option added to reduce the number of grid square digits in the log after a HamQTH.com or qrz.com query: Preferences–>Databases
- New: Oceania DX Contest
- New: Pennsylvania QSO Party
- New: Russian World Wide Digital Contest
- New: California QSO Party
- New: RSGB International DX Contest
- New: Deutscher Telegraphie-Contest
- New: UK/EI DX Contest
- New: The Makrothen Contest
- New: JARTS WW RTTY CONTEST
- New: CQ WW DX Contest RTTY

#### 2.13.1 1-October-2016

- Fixed: Heading needle works again
- Fixed: Bug in PA QSO Party prior 10.10 users fixed
- Change: qrz.com queries ignore /P, /M, /AM, /MM and /QRP only, when the full call was not found

#### 2.14 27-October-2016

- New: FT-920 support
- New: TS-850 support
- New: IC-7300 - Scope, Macros and audio switching in the IC-7300 control window
- New: NRRL Telefoni Contest

#### 3.0 26-November-2016

- Fixed: Contest - Callsign check will be performed now after clicking in band map or dx-spot window - Tnx EA3HOE
- Change: TRX control macros for Elecraft will be stored now per model (K3, KX3, KX2)
- New: Support for new Touch Bar
- New: CQ marker in contest band map
- New: QSL label Avery 3658 (33.8 mm x 64.6 mm auf DIN A4 3 x 8)
- New: Köln-Aachen Herbstcontest (DARC)
- New: ARRL Sweepstakes contest
- New: HA-DX Contest

#### 3.1 28-December-2016

- Fixed: Station Info Box shows correct distance now when english units are used - Tnx KH6BE
- Fixed: Printing 60m QSLs without a Crash now - Tnx DK5LP
- Fixed: Scrolling in the log using the arrow keys works doesn’t cause the app to crash - Tnx N9JR
- Change: New rules for the Helvetia Contest implemented
- Change: New rules for the NAQP implemented
- New: A row for the QSO serial number can be shown in the log table now. These number is valid for the seen QSOs only!
- New: QSL label format Avery 5363 (2-13/16" x 1-3/8" at US Letter, 3 x 8)
- New: Changes made for latest microHAM firmware updates (MKII: 6.7, DKII: 3.6)
- New: Added few Apple Script commands required for JT-Bridge, see function library
- New: Support for 60m added in:
  - Station Info Box
  - DXCC Info Box
  - Paper QSL In Info Box
  - Paper QSL Out RIG Text
  - DXCC List and counter
  - DX cluster

#### 3.2 23-January-2017

- Fixed: Fixed a problem while saving a QSO with suspecting content in the Manager or US-County field - Tnx K3URT & DJ6GI
- Fixed: The US-County selection is kept now when tabbing into the State field - Tnx VA2SS
- Fixed: Minor problem with dx-cluster macros - Tnx VA2SS
- New: Support for FT-1000D (ROM version 6 required)
- New: QSL Label (38.1 mm x 70 mm mm auf DIN A4, 3 x 7)
- New: Row for 4m in the Grid Square table added
- New: In the Search QSOs window can be searched for QSOs with a specific color code
- New: When you make a recording for the voice keyer, you can optionally overwrite an existing file: Overwrite existing file
- New: FSK and CW messages can be started global using the F-keys: Preferences–>microHAM
- New: The local time of the dx station is shown now (macOS 10.11 or newer required)
- New: AGCW Happy New Year Contest
- New: ARRL VHF Contests (January, June, September) - 6m, 2m, 1.25m, 70cm, 33cm, 23cm and 13cm only
- New: DARC Februar QSO Party
- New: DARC UKW-Winter-Fieldday

#### 3.2.1 24-January-2017

- Fixed: Crash when using an older macOS version - Tnx K3URT
- New: TRX control windows: clicking on a frequency read out digit, increments or decrements this digit

#### 3.3 28-February-2017

- Fixed: Some functions didn’t worked as expected in the IC-7300 Control Window on non Europain systems - Tnx K0PIR
- Fixed: Refresh of the Sun Window works more reliable now
- New: Real time callsign check sheet: Menu–>Contest–>Callsign check sheet
- New: Map to show worked grid squares in VHF contests: Menü–>Contest–>Show grid map
- New: QSL label Avery 3422 (35 mm x 70 mm at DIN A4 3 x 8)
- New: Band maps support 60m now (except contest), but no mode recognition
- New: Transceiver clock setting for the IC-7300 (IC-7300 Ctrl window)
- New: Changes made for ADIF version 3.0.5, mainly new operating modes
- New: Wisconsin QSO Party
- New: Oklahoma QSO Party
- New: DARC UKW-Sommer-Fieldday
- New: DARC UKW Frühlingswettbewerb
- New: DARC VHF-, UHF-, Microwave Contest March
- New: DARC VHF-, UHF-, Microwave Contest May
- New: DARC VHF-, UHF-, Microwave Contest June
- New: DARC VHF-, UHF-, Microwave Contest July
- New: IARU-Region-1 145 MHz Contest September
- New: IARU-Region-1 UHF/Microwaves Contest October
- New: Nordic Activity Contest

#### 3.4 28-April-2017

- New: Dx-Spot-Window - The background of the Age column is different colours now to visualize the age of the spot
- New: Satellite list updated
- New: TS-990 support
- New: Log window: When the option Real Time isn’t checked, the background of the date and time fields change to orange - just an eye catcher
- New: Naval Day Contest
- New: AGCW QRP-QRP Contest
- New: Save complete ADIF files via AppleScript, useful for Fldigi users - See FAQ
- New: Network functions added (not for the contest interface yet)

#### 3.4.1 29-April-2017

- Fixed: Bug fixed for the Helvetia contest, HB9 stations were affected only - Tnx Gerald, HB9CEY

#### 3.4.2 01-May-2017

- Fixed: The US-States window works again - Tnx Bob, KH6BE

#### 3.5 06-June-2017

- Fixed: SOTA dx-cluster elgur.dtdns.net works now - Tnx Michael, KX6A
- Fixed: The US-County window works again
- Fixed: The Search QSOs window didn’t show any search options after a clean install - Tnx Robin, G4GIY
- New: Support for Kiwi SDR
- New: Support for FT-891
- New: Option added to overwrite a QSO partially during an ADIF import
- New: Support for verified DXCC- and IOTA credits

#### 3.5.1 11-June-2017

- Fixed: A problem with the 6m band map

#### 3.6 15-July-2017

- Change: LoTW user data are loaded from the ARRL site now
- New: Club Log users with an online log and/or OQRS are marked in the Station Info Box
- New: Club Log user data are shown in the HamQTH/qrz.com table
- New: New Command for all QSO tables: Menu–>QSO–>Select stations using OQRS (Club Log OQRS)
- New: Option Preferences–>DX cluster–>Transfer spot note to logging field ‘Note’
- New: Award tables can be sorted by band
- New: Menu entry to open a recently used logbook or contest
- New: Ex- and Import functions in ADX format
- New: Another DXCC status overview below the DXCC-Info-Box
- New: ARRL 222 Mhz and up distance contest (ARRL UHF August contest)
- New: Marconi Memorial CW Contest
- New: CQ WW VHF Contest
- New: MOON Contest

#### 3.6.1 17-July-2017

- Fixed: Failure in DXCC computation, caused the app to quit working without crashing after few thousands of calculations - Tnx Siso, HK3W

#### 3.7 24-August-2017

- Fixed: IOTA color coding in the dx spot window - Tnx Thomas, DL1AMQ
- Fixed: Contest interface - shown report (rx+tx) was sometimes different from the saved report Tnx Radek, OK2VBZ
- New: Hamqth/qrz.com side panel added to the contest window
- New: Interfaces to WSJT-X
- New: Store audio, graphic or text data in your log database.
- New: Changes for ADIF 3.0.6 (new modes and submodes, support for the tag <DARC_DOK>
- New: SSA Monthly Contest
- New: South America Sprint Contest

#### 3.8 29-September-2017

- Change: A dx spot already worked in this slot will not be announced again via notification or voice
- Fixed: DX-Spot are shown correct when RUMlog uses local time - Tnx Mattia, IZ3WTP
- Fixed: On a system, where RUMlog was never running, it was not possible to open an already existing logbook file - Tnx Andy, DL1AKP
- New: Option added in the dx-spot window to hide already worked stations
- New: IC-7300 control window shows the manual notch filter frequency
- New: Solar Activity Status Window (http://www.n3kl.org/sun/status.html)
- New: Support für Spanish TPEA award
- New: New York QSO Party
- New: Iowa QSO Party
- New: Illinois QSO Party
- New: Thüringen Contest

#### 3.8.1 4-October-2017

- Fixed: A crash when WSJT-X reports just a single word in a message -Tnx David, VK3LDB
- Fixed: Pennsylvania QSO Party allows now to enter more then one Bonus station - Tnx John Miller

#### 3.9 9-December-2017

- Fixed: Freezing Fldigi - Tnx JC, W6IPA for great assistance
- Fixed: 10m band added to the NAC (contest) and EDI log corrected (claimed score includes now the bonus points) - Tnx Hans, SM6BNA
- Fixed: Bug with the macros in the CW window - Tnx Andy, DL1AKP
- Fixed: PSK mode switching for TS-570 - Tnx David, VA3CP
- New: Support for keyboard modifiers while double clicking on a WSJT-X dx-spot (WSJT-X 1.8 rc3 or newer required)
- New: HSW Aktivitätswettbewerb (Local German contest)

#### 3.10 23-January-2018

- Fixed: HTTP Error 404 for few download functions
- Fixed: Corrections were made in the logbook, since LoTW returns ITU and cq zone numbers with a leading zero
- Fixed: Crash when Club Log data are corupted - Tnx Jason, N4JJS
- New: Stew Perry Topband Distance Challenge
- New: Changes for microHAM MKII firmware 6.12 und DKII firmware 3.8
- New: (WSJT-X) CQ answer for new ones (FT8 only)

#### 3.10.1 25-January-2018

- Fixed: Data Mode switching in the IC-7300 Control panel

#### 3.11 14-March-2018

- Fixed: “Hide non worked entities” option in the dxcc list works correct again - Tnx Bob, AA6OC
- New: ADIF SIG and SIG_INFO tags for user fields added
- New: List of Satellites updated
- New: Text colour for New ones below the DXCC Status Box are free selectable: Preferences–>DX-Alarm–>Select Colours
- New: Spanish translation - Tnx Alfonso, EA5725URE
- New: IC-7610 control panel
- New: IC-7610: Auto discovery of the used USB port

#### 3.11.1 18-March-2018

- Fixed: Minor bug concerning multipliers for OK-QP and WI-QP - Tnx Mark, NX1K
- Fixed: Independent Cities in Virginia added to the County list - Tnx Bob, AA6OC
- New: Support for Dymo Labelwriter format 89mm x 41mm

#### 3.12 20-April-2018

- Fixed: Missing DXCC list update for LoTW QSLs in some cases - Tnx Clarke, K1JX
- New: Portuguese translation - Tnx David, CT1DRB
- New: Support for Italian provinces (WAIP award)
- New: AppleScript function to get recently logged QSOs in ADIF or ADX format
- New: Extra network settings for the contest module
- New: Support for the QSO Upload Utility
- New: RSGB UKAC Contest
- New: HSC Contest
- New: International Naval Contest
- New: CQMM DX Contest (ex Manchester Mineira All America CW Contest)
- New: WFDA Winter Field Day
- New: Ohio QSO Party
- New: Michigan QSO Party

#### 3.12.1 30-April-2018

- Fixed: All UDP settings are saved now - Tnx Mike, KB3LAN
- Fixed: After showing CQ or ITU Zones tables, the database was locked for write operations - Tnx Dana, VE3DS
- Fixed: Crash in the WPX window - Tnx Alexander, DG0OJO
- Fixed: Crash while opening existing logbook files
- New: WSJT-X: Color coding for callsigns WSJT-X version 1.9 RC4 or newer required!
- New: IC-7610 Ctrl. window: Option added to correct the scope reference level according the scope band width
- New: CAT TCI Interface for Expert Electronics devices- Tnx Rick, VE3MM & Björn, SM0MDG

#### 3.12.2 22-May-2018

- Fixed: Crash when viewing prev. QSOs - Tnx Charles, NK8O & Terry, M0CLH
- Fixed: Problems with the K3 PSK mode setting when using the K3 Ctrl panel - Tnx Mike, K9JRI

#### 4.0 24-September-2018

The IC-7610 Auto Discovery function doesn’t work under macOS 10.13 High Sierra!

- Changed: Alle drawer type panels are now “normal” windows (HamQTH/qrz.com, RTTY, multiplier help) due to missing support in upcoming macOS versions
- Changed: Manual saving of QSOs from WSJT-X
- Changed: macOS 10.13 (High Sierra) or newer required
- Deleted: Growl support removed, due to missing 64bit supoort
- Deleted: Import of RUMlog Classic logbook files
- New: Support for Dymo Labelwriter 90mm x 38mm
- New: Support for label format Avery 3477
- New: Support “Dark Mode” in Mojave
- New: DXCC Entity table shows headings and directions
- New: Data take over from the HamQTH/qrz.com result table to the Edit QSO entry mask
- New: Touchbar support in the IC-7610 control panel
- New: In WSJT-X saved QSOs can be saved in the Contest log useful for Dx-Peds
- New: Filter options in the contest DX-Spot window (FT-8 frequencies are fixed)
- New: FT8 mode recognition for DX-Cluster spots (FT-8 frequencies are fixed
- New: New ADIF tags <TEN_TEN> and for user definable logging fields
- New: Optional use of macOS location services whenever the own grid square needs go be entered
- New: Scope for IC-7610/IC-7300 shows more control options
- New: Contest Scoreboards
- New: Level slider in theIC-7300 Control Panel
- New: DMC RTTY Contest
- New: Russian translation started - Tnx Vladimir, R2ADU

#### 4.0.2 28-September-2018

- Fix: Crash while opening the *Preferences Window**

#### 4.0.3 12-October-2018

- Fix: Crash while opening the Preferences Window
- New: IC-7610 Control Panel: IF band width, Shift, notch filter and AGC settings are shown now for the Sub RX

#### 4.0.4 16-October-2018

- Fix: Crash when using the IC-7610 Ctrl Window - Tnx Terry, M0CLH & John, N1JM
- New: WinKeyer - Control slidfer for QSK compensation added
- New: DX voice announcements can be limited to avoid the same announcement in a given time interval: Preferenecs–>DX Alarm–>Spoken DX Spots
- New: After saving a QSO from WSJT-X, the text colour of the affected station will be reset

#### 4.0.5 11-November-2018

- Fix: Autolayout failure in the Contest Window** and in the Contest Info Panel* - Tnx Andy, DL1AKP & Georg, DJ6GI
- Fix: Fldigi crashes
- New: Announce DX-Spotsfrom the Contest Window

#### 4.1 20-January-2019

- Fix: Contest Scoreboard Windows don’t get any longer the focus - Tnx David, CT1DRB
- New: Added a menu entry for HamQTH/qrz.com/CQQRZ Info Window
- New: Support qrzcq.com
- New: JS8 Mode added (ADIF version 3.0.9)
- New: Transceiver support TenTec Omni VII
- New: QSO Note field can be added to the SOTA export
- New: Contest support for WSJT-X QSOs
- New: WSJT-X can overwrite user definable logging fields in the QSO record if applicable (my_gridsquare, time_on, operator, station_callsign)
- New: ADIF/ADX Export for special activities (WWFF)
- New: Option for the FT-8x7 added to change the mode automatically for voice keyer operation - SSB-DIG-SSB
- New: NRAU-BALTIC Contest
- New: ES-OPEN HF Championship
- New: BARTG Sprint Contest (also used for BARTG Sprint 75 Contest)
- New: BARTG HF RTTY Contest

#### 4.2 1-April-2019

- Fix: Format issue in WSJT-X Spots with enabled option Menu–>Decode–>Enable AP - Tnx Federico, IW0RBS
- Fix: Crash when starting the contest WIQP (Wisconsin side) - Tnx Joe, N9JR
- New: Support for JTDX (alternate for WSJT-X)
- New: List of satellites updated
- New: Contextual menus for often used function in QSO und DX-Spot tables added
- New: WSJT-X colours for callsign colour coding adjusted
- New: Option added to log QSO start or end time
- New: The WSJT-X windows will be cleared when changing the band - WSJT-X 2.0.1 required
- New: Mexico RTTY International Contest
- New: National CW Contest (URE CNCW)

#### 4.3 12-June-2019

- New: Icom Scope windows renewed
- New: IC-9700 support, includin control and & scope
- New: Avery 4738 (70 mm x 50,8 mm auf DIN A4 2 x 5)
- New: FT4 (MFSK sub mode)
- New: Support Red Pitaya (Stemlab) FT8 Skimmer
- New: Ontario QSO Party
- New: AGCW DL VHF/UHF Contest
- New: IARU Region 1 6m/4m Contest

#### 4.3.1 12-July-2019

- Fix: Crash when minimizing the waterfall in the Icom Scope Window - Tnx John, N1JM
- Fix: Crash when using Fldigi 4.1.05 - Tnx Jens, DL7AUO
- Fix: Failure in the ADIF import, when using non ASCII characters - Tnx Yuzo, JR1GDY
- New: Washington State Salmon Run

#### 4.3.2 13-July-2019

- Fix: Wrong usage of WSJT-X qso data for some configurations - Tnx Pavol, OM0WT
- New: Grid Square added to the Contest Cheat Database - Please reload: Menu–>Online

#### 4.4 18-September-2019

- Fix: Unwanted scope mode switching (IC-7300/7610/9700) - Tnx Terry, M0CLH
- Fix: Rule changes for the Pennsylvania QSO Party added
- Fix: ITU Zone for CE corrected
- Fix: ADIF tag prop_mode added for satellite QSOs to the eQSL upload
- Fix: Satellite QSOs will be clearly marked on printed QSL labels
- New: Changes in the DXLab Suite Commander Server for more flexibility when using two transceivers
- New: Autodiscovery function for the IC-9100
- New: Contextual menu added to the contest interface QSO table
- New: SCC RTTY Championship
- New: SARTG WW RTTY Contest
- New: WW Digi Contest

#### 4.4.1 10-October-2019

- Fix: Bug in Icom Auto Discovery when you have connected two Icom transceivers - Tnx Wolfgang, DL1IE
- Fix: Bug in the TCI CAT protocol - Tnx Frank, DF8FF
- Fix: Bug in the DXLab Suite Commander Server - Tnx Mat, LA0FA
- New: Support for qrz.ru

#### 4.5 10-December-2019

- Fix: Initialization error K1EL Winkeyer - Tnx Bruce, W4CG
- Fix: PTT for Contest Voice Keyer - Tnx Jan-Henrik, DK1OM
- Fix: Cabrillo Soapbox - Tnx Jan-Henrik, DK1OM
- Fix: Default ITU Zone for CP changed to 14 - Tnx Francesco, IV3TMM
- New: Transverter support for TRX#1 und TRX# 2
- New: Support Avery 4780 (48,5 mm x 25,4 mm at DIN A4 4 x 10)
- New: Support Avery 6032 (63,5 mm x 33,9 mm at DIN A4 3 x 8)
- New: Unterstützung Club Log Gateway (real-time uploads)
- New: No CAT data update when Manuel time entry is selected
- New: Third App Auto Start feature
- New: Russian World Wide MultiMode Contest

#### 4.5.1 22-Ferbruary-2020

- Fix: New rules for HA-DX Contest included - Tnx David, CT1DRB and John, K8AJS
- Fix: CQ-WW-160 fixed for W stations - Tnx Ryan, NN7M
- Fix: Changes made for cqcontest.net and contestonlinescore.com
- New: Eurasia Championship

#### 4.6 4-April-2020

- Fix: ITU zones corrected for TI9 and VP8 - Tnx Francesco, IV3TMM
- New: flrig can be used for CAT
- New: Funktion added to find dupe QSOs in the logbook: Menü–>QSO–>Show dupes (callsign, band, mode, date, time )
- New: QSL label Avery 3651 (52,5 mm x 29,7 mm at DIN A4 4 x 10)
- New: The Frisian Eleven Cities Contest
- New: DARC Funk.Tag Contest
- New: RSGB Hope QSO Party

#### 4.7 15-May-2020

- New: All K7PT functions removed, since this service is not any longer available
- New: Data exchange with JS8Call
- New: Support for multiple transceiver configuration settings
- New: CAT On/Off switch in Menu–>Transceiver
- New: Multiple CW, RTTY and Phone memory settings (Logbook & Contest)
- New: Supports RTTY for WinKeyer since version 3.1
- New: Use of the WinKeyers Pushbuttons as keypad for RUMlog
- New: Auto Start function for the audio file recorder
- New: user selectable band map colours: Preferences–>DX Alarm–>Select Colours
- New: Satellite list user editable Preferences–>Modes/Sat
- New: CQ-Zone recognition with help of Club Log databases
- New: Hessen contest updated and VHF part added