| # DXLab Suite Commander Server

RUMlog offers three DXLab servers internally. One turned on by ticking the checkbox on the TX 1 preference pane, a second one in TX 2, and a third one toggles between the transceivers. You can connect two transceivers, but only one will affect RUMlog at a time.

Do not activate a server in WSJT-X and in TRX settings at the same time.

Currently only a subset of the available commands are supported. Split functions are not supported yet. Please contact me if you require additional functions to be supported.

# See Also

WSJT-X/JTDX/JS8Call and RUMlog