| # IC-9700 Control

The functions are very similar to the IC-7300/7610 control panels, please read that section for more information. Please note: Use the fastest available USB connection (115200 baud).

If RUMlog is allowed to access your current location it can send it to IC-9700.

The Auto Repeater function is supported. The repeater offset can be selected automatically according to the IARU region 1 band plan. This function is available for 2 m and 70 cm bands.

Weather data can be sent from a Netatmo weather station to the transceiver. It requires a separate serial connection to the transceiver’s Data socket. The speed is fixed at 9600 baud. Make sure to configure your transceiver accordingly.

# See Also

Icom Remote Encoder RC-28

IC-7300 Control Panel

IC-7610 Control Panel

Scope IC-7610

Icom Auto Discovery

# External Links

Netatmo weather station