| # Station Info Box

Various error and status information appears just above the box.

The information in the box is similar to the DXCC Info Box. A callsign in magenta indicates an invalid operation. Accurate sunset and sunrise times, and bearing and distance information are available only if the correct location has been given in the Locator field.

To indicate a Club Log LoTW or eQSL AG member, you have to first load the user lists in: Menu–>Online.

Click the mouse in the box to show all the QSOs with this station in the logbook table.

The box shows OQRS if the station offers a OQRS in Club Log. If there is only an online log available, the box shows CL.

The local time of the dx station can be shown between the DXCC and Station Info Box. If the exact position is known (HamQTH.com, qrzcq.com, or qrz.com) the time readout appears in blue. If not, the default DXCC position will be used and the time text color is brown.
An internet connection is always required for this service.

The Station Info Box is used for dropping files you want to save with in your logbook database file.

# See Also

Save and view multi media data